SPECjbb2013
Copyright © 2012-2013 Standard Performance Evaluation Corporation

Poseidon Technologies STAR T2 | INVALID RESULT: 55193 SPECjbb2013-MultiJVM max-jOPS 18467 SPECjbb2013-MultiJVM critical-jOPS
Tested by: Neptune Corp. (Willie Cando) | Test Sponsor: ABC Corp | Test location: Santa Monica, CA | Test date: Apr 25, 2005
SPEC license #: 50 | Hardware Availability: May-2000 | Software Availability: May-2000 | Publication: MMM DD, YYYY

Validation Errors Summary
Validation level CORRECTNESS is missing from the Validation Reports
Benchmark Results Summary

SPECjbb2013-MultiJVM: Multiple JVMs/Single Host (# of groups: 2) Overall SUT Description SUT Description max-jOPS and critical-jOPS Details Number of probes Request Mix Accuracy Rate Of Non-Critical Failures Delay between performance status pings IR/PR Accuracy Topology SUT Configuration Properties Validation Details | Overall Throughput RT curve

Overall SUT (System Under Test) Description

Vendor | Poseidon Technologies
Vendor URL | http://poseidon.com/
System Source | Single Supplier
System Designation | Server Rack
Total Systems | 1
All SUT Systems Identical | YES
Total Nodes | 8
All Nodes Identical | YES
Nodes Per System | 8
Total Chips | 16
Total Cores | 32
Total Threads | 64
Total Memory Amount (GB) | 8
Total OS Images | 1
SW Environment | Non-virtual

SUT Description

Hardware hw_1
Vendor | Poseidon Technologies
Vendor URL | http://poseidon.com/
Available | May-2000
Model | STAR T2
Form Factor | Tower etc.
CPU Name | Intel Xeon 2350M
CPU Characteristics | Quad-Core, 2.50GHz, 8MB L3 Cache (Turbo Boost Technology up to 3.50 GHz)
Number of Systems | 1
Nodes Per System | 4
Chips Per System | 4
Cores Per System | 4
Cores Per Chip | 4
Threads Per System | 4
Threads Per Core | 4
Version | V33.333 patch-level 78
CPU Frequency (MHz) | 2998
Primary Cache | 16KB(I)+16KB(D) per core
Secondary Cache | 128 KB (I+D) per core
Tertiary Cache | 4MB (I+D) on chip per chip
Other Cache | None
Disk | 2x 300GB 10K RPM, see notes
File System | UFS
Memory Amount (GB) | 8
# and size of DIMM(s) | 2 x 4096MB
Memory Details | 2Rx8 PC3L-12800E ECC CL11; slots 1A, 1B populated
# and type of Network Interface Cards (NICs) | 3x 10 Gbit NICs
Power Supply Quantity and Rating (W) | 3 x 550
Other Hardware | 4x Sun 8Gb FC Dual GbE HBA ExpressModule
Cabinet/Housing/Enclosure | None
Shared Description | None
Shared Comment | None
Tuning | None
Notes | None
Other Hardware network_1
Vendor | Poseidon Technologies
Vendor URL | http://poseidon.com/
Version | V33.333 patch-level 78
Available | May-2000
Bitness | n/a
Notes | None
Operating System os_1
Vendor | Poseidon Technologies
Vendor URL | http://poseidon.com/
Version | V33.333 patch-level 78
Available | May-2000
Bitness | 64
Notes | None
Java Virtual Machine jvm_1
Vendor | Phobos Ltd
Vendor URL | http://www.phobos.uk.com
Version | JDK 7 update 3
Available | Jan-2000
Bitness | 64
Notes | note
Other Software other_1
Vendor | Poseidon Technologies
Vendor URL | http://poseidon.com/
Version | V33.333 patch-level 78
Available | May-2000
Bitness | 64
Notes | None

max-jOPS and critical-jOPS Details

max-jOPS = jOPS passed before the First Failure
Pass/Fail | Pass | Pass | Pass | Pass | Pass
jOPS | 52844 | 53432 | 54019 | 54606 | 55193
critical-jOPS = Geomean ( jOPS @ 10000; 50000; 100000; 200000; 500000; SLAs )
Response time percentile is 99-th
SLA (us) | 10000 | 50000 | 100000 | 200000 | 500000 | Geomean
jOPS | 7926 | 10862 | 16146 | 32685 | 47266 | 18467
| Last Success jOPS/First Failure jOPS for SLA points
| Percentile
| 10-th | 50-th | 90-th | 95-th | 99-th | 100-th
500us | - / 587 | - / 587 | - / 587 | - / 587 | - / 587 | - / 587
1000us | - / 587 | - / 587 | - / 587 | - / 587 | - / 587 | - / 587
5000us | 46386 / 46973 | 35230 / 35817 | 4110 / 4697 | 3523 / 4110 | 2349 / 2936 | - / 587
10000us | 48147 / 48734 | 44037 / 44624 | 28184 / 28771 | 19963 / 20551 | 7633 / 8220 | - / 587
20000us | 49321 / 49909 | 44624 / 45211 | 33468 / 32881 | 25248 / 25835 | 9982 / 10569 | 587 / 1174
50000us | 49321 / 49909 | 45798 / 46386 | 34642 / 35230 | 26422 / 27009 | 11156 / 10569 | 1761 / 1174
100000us | 49909 / 50496 | 46386 / 46973 | 38165 / 36404 | 33468 / 32294 | 16440 / 15853 | 1761 / 1174
200000us | 50496 / 51083 | 48147 / 48734 | 44624 / 45211 | 42276 / 36404 | 33468 / 32294 | 14092 / 1174
500000us | 53432 / 52844 | 51083 / 51670 | 48147 / 48734 | 47560 / 48147 | 46973 / 47560 | 33468 / 32881
1000000us | 55193 / - | 54019 / 54606 | 52257 / 52844 | 51670 / 52257 | 49909 / 49321 | 42276 / 36404

Number of probes

Request Mix Accuracy

Note (Actual % in the Mix - Expected % in the Mix) must be within: 'Main Tx' limit of +/-5.0% for the requests whose expected % in the mix is >= 10.0% 'Minor Tx' limit of +/-1.0% for the requests whose expected % in the mix is < 10.0%

Rate of Non-Critical Failures
There were no non-critical failures in Response Time curve building
Delay between performance status pings during RT Curve (Response-Throughput Curve)

IR/PR Accuracy
Topology

- SUT
  - Hardware config_1
    - OS Image os_Image_1
      - JVM jvm_Ctr_1 : Controller
      - JVM jvm_Backend_1 : Backend
      - JVM jvm_TxInjector_1 : TxInjector

SUT config_1 Configuration

Hardware
OS Images | os_Image_1(1)
Hardware Description | hw_1
Number of Systems | 1
SW Environment | non-virtual
Tuning | tuning
Notes | notes
OS Image os_Image_1
JVM Instances | jvm_Ctr_1(1), jvm_Backend_1(4), jvm_TxInjector_1(4)
OS Image Description | os_1
Tuning | bufcache=1024 threads=65536
Notes | None
JVM Instance jvm_Ctr_1
Parts of Benchmark | Controller
JVM Instance Description | jvm_1
Command Line | -ms256m -mx1024m
Tuning | affinity note 1 note 2
Notes | "Notes here"
JVM Instance jvm_Backend_1
Parts of Benchmark | Backend
JVM Instance Description | jvm_1
Command Line | -Xms24g -Xmx24g -Xmn20g
Tuning | affinity note 1 note 2
Notes | "Notes here"
JVM Instance jvm_TxInjector_1
Parts of Benchmark | TxInjector
JVM Instance Description | jvm_1
Command Line | -Xms2g -Xmx2g
Tuning | affinity note 1 note 2
Notes | "Notes here"

Run Properties

This section lists properties only set by user; use -defaultProps reporter option to list all properties
Property Name | Default | Controller
specjbb.group.count | 1 | 2
specjbb.txi.pergroup.count | 1 | 1
View table in csv format

Validation Details
Validation Reports

Level: COMPLIANCE
Check | Agent | Result
Check properties on compliance | All | PASSED

Other Checks
High-bound (max attempted) is 58716 IR
High-bound (settled) is 56876 IR

Copyright © 2012-2013 Standard Performance Evaluation Corporation
http://www.spec.org - info@spec.org
SPECjbb2013 Version: [SPECjbb12013 1.0, October 24, 2012]