< prev index next >

## src/cpu/x86/vm/macroAssembler_x86.hpp

Print this page

    @@ -1239,10 +1239,29 @@
                                    Register yz_idx, Register idx, Register jdx,
                                    Register carry, Register product,
                                    Register carry2);
       void multiply_to_len(Register x, Register xlen, Register y, Register ylen, Register z, Register zlen,
                            Register tmp1, Register tmp2, Register tmp3, Register tmp4, Register tmp5);
    +
    +  void square_rshift(Register x, Register len, Register z, Register tmp1, Register tmp3,
    +                     Register tmp4, Register tmp5, Register rdxReg, Register raxReg);
    +  void multiply_add_64_bmi2(Register sum, Register op1, Register op2, Register carry,
    +                            Register tmp2);
    +  void multiply_add_64(Register sum, Register op1, Register op2, Register carry,
    +                       Register rdxReg, Register raxReg);
    +  void add_one_64(Register z, Register zlen, Register carry, Register tmp1);
    +  void lshift_by_1(Register x, Register len, Register z, Register zlen, Register tmp1, Register tmp2,
    +                       Register tmp3, Register tmp4);
    +  void square_to_len(Register x, Register len, Register z, Register zlen, Register tmp1, Register tmp2,
    +                     Register tmp3, Register tmp4, Register tmp5, Register rdxReg, Register raxReg);
    +
    +  void mul_add_128_x_32_loop(Register out, Register in, Register offset, Register len, Register tmp1,
    +               Register tmp2, Register tmp3, Register tmp4, Register tmp5, Register rdxReg,
    +               Register raxReg);
    +  void mul_add(Register out, Register in, Register offset, Register len, Register k, Register tmp1,
    +               Register tmp2, Register tmp3, Register tmp4, Register tmp5, Register rdxReg,
    +               Register raxReg);
     #endif

       // CRC32 code for java.util.zip.CRC32::updateBytes() instrinsic.
       void update_byte_crc32(Register crc, Register val, Register table);
       void kernel_crc32(Register crc, Register buf, Register len, Register table, Register tmp);

< prev index next >