# Layout - Drying

In this page you can access all the drying system related devices

In every page you can see 3 different dryers.

On the right of every dryer there are all the hoppers assigned to that specific dryer.

If on the right the arrow is visible that means that you can cycle through all the other hoppers assigned that now are not visible.

On the bottom is possible to see these buttons and status

If the right/left arrow is visible that means that you can cycle through all the other dryers that now are not visible.

## Gmp dryer

The Gmp dryer device rappresentation contains several functions and status icon:

| This is the clickable part that brings you to the device detail. The device can be drawn in different color: - BLUE if the dryer is offline (no communication) - GRAY if the dryer is stopped - GREEN if the dryer is now started - YELLOW if the dryer is in cooling stop state
| All additional status are shown with these icons: - Alarm Icon: 1) GRAY if there’s no alarm 2) RED if there’s at least 1 alarm
| The dryer assigned name
| The dryer status: - Started - Stopped - Cooling stop
| By clicking the command button this popup will be shown. Here the list of command available: - Start allow you to enable the dryer - Stop allow you to disable the dryer

## Gmp hopper

| The device can be drawn in different color: - BLUE if the hopper is offline (no communication) - GRAY if the hopper is disabled - GREEN if the hopper is now enabled
| All additional status are shown with these icons: - Alarm Icon: 3) GRAY if there’s no alarm 4) RED if there’s at least 1 alarm - Dehum material: 1) GRAY if the material is dehumified 2) RED if the material need more time to get ready
| The hopper assigned name
| The gmp hopper parameters “Set point” and “Process temperature”
| By clicking the command button this popup will be shown. Here the list of command available: - Start allow you to enable the hopper - Stop allow you to disable the hoppper