# Layout - Loading

In this page you can access all the loading system related devices

In every page you can see 3 different pump.

On the right of every pump al the stations assigned to that specific pump are shown.

If on the right the arrow is visible that means that you can cycle throught all the other stations assigned that now are not visible.

On the bottom is possible to see these buttons and status

FACS-X Loading System allow you to start and stop the whole loading system.

If the right/left arrow is visible that means that you can cycle throught all the other pump that now are not visible.

## Loader pump

The pumps device rappresentation contains several functions and status icon:

| This is the clickable part that brings you to the device detail. The device can be drawn in different color: - BLUE if the pump is offline (no communication) - GRAY if the pump is stopped - GREEN if the pump is now started
| All additional status are shown with these icons: - Alarm Icon: 1) GRAY if there’s no alarm 2) RED if there’s at least 1 alarm - Shutdown in progress: 1) GRAY there’s no shoutdown procedure active on this device 2) YELLOW if the device is shutting down because of the procedure 3) RED if there was a problem with the shutdown procedure - Filter pulse: 1) GRAY if is not active 2) GREEN if is now active - Motor running: 1) GRAY if is not running 2) GREEN if is now running - Vacuum breaker valve: 1) GRAY if is not energized 2) GREEN if is now energized
| The pump assigned name
| The pump status: - OFF if the pump is disabled - ON if the pump is enabled
| By clicking the command button this popup will be shown. Here the list of command available: - Start allow you to enable the pump - Stop allow you to disable the pump - Start group allow you to enable the pump and all the stations assigned - Stop group allow you to disable the pump and all the stations assigned

## Loader station

| The device can be drawn in different color: - BLUE if the station is offline (no communication) - GRAY if the station is disabled - GREEN if the station is now enabled
| All additional status are shown with these icons: - Alarm Icon: 1) GRAY if there’s no alarm 2) RED if there’s at least 1 alarm - Shutdown in progress: 1) GRAY there’s no shoutdown procedure active on this device 2) YELLOW if the device is shutting down because of the procedure 3) RED if there was a problem with the shutdown procedure - Station status: 1) GRAY is the station has no need to load material 2) ORANGE if the station is in queue waiting for load 3) GREEN if the station is now loading
| The station assigned name
| The station status: - OFF if the station is disabled - ON if the station is enabled
| By clicking the command button this popup will be shown. Here the list of command available: - Start allow you to enable the station - Stop allow you to disable the station