# Layout - Storage

In this page you can access all the storage related devices

In every page you can see a maximum of 12 storage devices.

On the bottom is possible to see these buttons and status

If the right/left arrow is visible that means that you can cycle throught all the other storage pages that now are not visible.

## Silo monitor

The silo monitor device rappresentation contains several functions and status icon:

| This is the clickable part that brings you to the device detail. The device can be drawn in different color: - BLUE if the silo monitor is offline (no communication) - GRAY if the silo monitor is connected The progressbar rappresent the material level inside the silo
| All additional status are shown with these icons: - Alarm Icon: 1) GRAY if there’s no alarm 2) RED if there’s at least 1 alarm - Sounding: 1) GRAY if the procedure is not active 2) YELLOW is the procedure is requested 3) GREEN if the procedure is in progress 4) RED if the procedure failed
| The silo monitor assigned name

## Non networked devices

The non networked device rappresentation contains several functions and status icon:

| This is the clickable part that brings you to the device detail. The icon can change and the user can choose the right icon that fits the selected device
| The non networked device assigned name

##