# Layout - Dosing

In this page you can access all the dosing system related devices

In every page you can see a maximum of 12 dosers per page.

On the bottom is possible to see these buttons and status

If the right/left arrow is visible that means that you can cycle throught all the other doser pages that now are not visible.

## Quantum

The pumps device rappresentation contains several functions and status icon:

| This is the clickable part that brings you to the device detail. The device can be drawn in different color: - BLUE if the quantum is offline (no communication) - GRAY if the quantum is stopped - GREEN if the quantum is now started
| All additional status are shown with these icons: - Alarm Icon: 1) GRAY if there’s no alarm 2) RED if there’s at least 1 alarm - Dosing: 1) GRAY if is not dosing 2) GREEN if the dosing procedure is now running
| The quantum assigned name
| The quantum status: - OFF if the quantum is disabled - ON if the quantum is enabled - Dosing if the quantum is now dosing
| By clicking the command button this popup will be shown. Here the list of command available: - ???? WAIT INFO FROM LORIS